

**Cruise Control Cable Replacement**

**[Removal Procedure](https://gsi.ext.gm.com/gsi/showDoc.do?docSyskey=629709&cellId=10812&pubObjSyskey=4234433&from=sm&pubCellSyskey=1345250&deliveryEffectiveDate=Aug+1%2C+2016" \l "d85356e3)**


1. Open the hood.

[lick here for detailed picture of the image.](https://gsi.ext.gm.com/gsi/showTif.do?image=276343)


1. Disconnect the cruise control cable tab (5) from the throttle body cam (6). Rotate the throttle to ¼ open throttle in order to release the tab (5).
2. In order to release the cable (4), push the locating fitting inward and pull the unit free from the throttle bracket (1).

[lick here for detailed picture of the image.](https://gsi.ext.gm.com/gsi/showTif.do?image=329483)

1. Remove the cable assembly from the module by turning the cable assembly ¼ turn counterclockwise.


[lick here for detailed picture of the image.](https://gsi.ext.gm.com/gsi/showTif.do?image=329482)

1. Remove the cable from the ribbon.


[lick here for detailed picture of the image.](https://gsi.ext.gm.com/gsi/showTif.do?image=276325)

1. Remove the cable (3) from the retaining clips (1).


[**Installation Procedure**](https://gsi.ext.gm.com/gsi/showDoc.do?docSyskey=629709&cellId=10812&pubObjSyskey=4234433&from=sm&pubCellSyskey=1345250&deliveryEffectiveDate=Aug+1%2C+2016#d85356e57)

[lick here for detailed picture of the image.](https://gsi.ext.gm.com/gsi/showTif.do?image=276325)

1. Install the cable (3) to the retaining clips (1).


[lick here for detailed picture of the image.](https://gsi.ext.gm.com/gsi/showTif.do?image=329482)

1. Install the cable to the ribbon.

[lick here for detailed picture of the image.](https://gsi.ext.gm.com/gsi/showTif.do?image=329483)

**Important:**Ensure that the ribbon does not become twisted when connecting the cable to the module.

1. Connect the cable assembly to the module by turning the cable assembly ¼ turn clockwise.



1. Install the cruise control cable tab (5) to the throttle body cam (6).
2. Align the cruise control cable fitting (4) to the throttle body bracket (1). Snap the fitting into place. Ensure that the fitting is retained.
3. Close the hood.

© 2016 General Motors.  All rights reserved.