**Steps for removing the intake manifold**

1. Disconnect Battery
2. Disconnect air filter from throttle body **(1 clamp)**
3. Unhook air filter, unscrew the air filter compartment **(6 screws)**
4. Unhook crankcase **(1 small screw)**
5. Unhook throttle body from intake manifold **(4 long bolts w/ washers)**
6. Unhook and cover pcv valve, brake booster, and EVAP **(Hoses + 1 clamp)**
7. Unhook tuning valve electrical + 1 other electrical connection on the top rear of the intake manifold
8. Unbolt 4 bolts on top of intake manifold **(1 on far right side, lower on the manifold; 3 on the rear of the manifold)**
9. Unbolt manifold from upper gaskets