1….(TCO 2) Type in the global configuration mode commands that will cause a user to be blocked for 10 minutes when three unsuccessful attempts are made to log in to the router within a time period of 2 minutes. (Points : 24)

2…. (TCO 3) Type the interface F0/10 commands that will shut down interface F0/10 if more than two MAC addresses are associated with interface F0/10. (Points : 24)

3…. (TCO 4) Discuss the two parameters that can be tracked by a CBAC firewall for TCP traffic that cannot be tracked for UDP traffic. (Points : 24)

4…. (TCO 5) Explain in detail the authentication methods in the following command. Also discuss the circumstances that will cause the next authentication method in the list to be used.  
aaa authentication login default group tacacs+ local enable (Points : 24)

5….. (TCO 6) Discuss the advantages and disadvantages of the following VPN technologies: GRE and L2TP. (Points : 24)

6….. (TCO 7) Explain the two benefits of Cisco IPS version 5.x signature format over the Cisco IPS version 4.x signature format. (Points : 22)

7….

|  |
| --- |
| (TCO 5) Which AAA server protocol offers support for ARAP and NETBEUI protocols as well as IP? (Points : 6) |

 CSACS  
       RADIUS  
       OpenACS  
       TACACS+