**Please keep in mind that I do not know your skill level on this subject, so I may be asking you questions for clarification purposes.**

**If the check engine light has come on, you will need to have the computer checked for codes. Most parts stores will do this for you at no charge for vehicles 1996 and up.**

**If the engine does not crank at all, check the battery and the cables first.**

**If the engine cranks but won’t start, check all the below items.**

* We need a strong blue spark at the plugs while cranking the engine
* We need GOOD COMBUSTIBLE fuel (take small fuel sample and light it)
* We need good fuel pressure and volume (tested with a GAGE)
* We need good compression (checking for broken timing belt or jumped chain)
* We need power to the injectors (checked using a NOID light only)
* We need unrestricted air to the intake and out the exhaust
* There must be (NO AIR LEAKS) after the MAF sensor to the throttle body (if applicable)
* BE SURE the security light is not on or flashing

**Please check ALL these items closely and with the proper tools**; it’s critical to our next steps!