
**Brake Pedal Position Sensor Replacement**

[**Removal Procedure**](https://gsi.ext.gm.com/gsi/showDoc.do?docSyskey=885355&cellId=79446&pubObjSyskey=4688945&from=sm&pubCellSyskey=1407625&deliveryEffectiveDate=Aug+1%2C+2016#d89170e3)

[lick here for detailed picture of the image.](https://gsi.ext.gm.com/gsi/showTif.do?image=1687770)

1. Remove the fuse block cover.
2. Disconnect the brake pedal position sensor electrical connector (1).
3. Remove the brake pedal position sensor bolts (2).
4. Remove the brake pedal position sensor (3) from the vehicle.

[**Installation Procedure**](https://gsi.ext.gm.com/gsi/showDoc.do?docSyskey=885355&cellId=79446&pubObjSyskey=4688945&from=sm&pubCellSyskey=1407625&deliveryEffectiveDate=Aug+1%2C+2016#d89170e41)

[lick here for detailed picture of the image.](https://gsi.ext.gm.com/gsi/showTif.do?image=1687770)

1. Install the brake pedal position sensor (3) to the vehicle.

**Notice:**Refer to [Fastener Notice](https://gsi.ext.gm.com/gsi/cellHandler.do?cellId=10105&refDoc=885355&from=sm) in Cautions and Notices.

1. Install the brake pedal position sensor bolts (2).  
   **Tighten**  
   Tighten the bolts to 9 Y (80 lb in).
2. Connect the brake pedal position sensor electrical connector (1).
3. Install the fuse block cover.