1995 JAGUAR XJ6 LEFT AND RIGHT HEELBOARD FUSEBOX

RIGHT SIDE POSITION

CONNECTOR A gauge NoMatch on Car CONNECTOR B gauge NoMatch on Car

POSITION 1 BrownOrg 10 X Brown Gray 10

POSITION 2 BrownYel 14 BrownOrg 14

POSITION 3 BrownRed 14 WhiteYel 14

POSITION 4 WhiteGray 14 WhitePink 14 X

POSITION 5 BrownBlk 10 BrownBlue 10 X

POSITION 6 BrownGray 10 BrownGreen 10

POSITION 7 BrownWhite 10 BrownGreen 10

POSITION 8 BrownPink 10 NOT USED

POSITION 9 WhiteRed 14 WhitePurple 14 X

POSITION 10 RedWhite 14 X BrownGreen 14

LEFT SIDE POSITION

CONNECTOR A gauge NoMatch on Car CONNECTOR B gauge NoMatch on Car

POSITION 1 BrownGray 10 BownPink 14 X

POSITION 2 BrownOrg 14 BrownPurple 14 X

POSITION 3 BrownRed 14 YellowWhite 14

POSITION 4 WhiteGray 14 BlueWhite 14

POSITION 5 BrownPurple 10 BrownWhite 10

POSITION 6 BrownGreen 10 BrownGreen 10

POSITION 7 BrownGreen 14 X BrownGreen 10

POSITION 8 BrownYellow 14 X NOT USED

POSITION 9 RedWhite 14 WhiteRed 14

POSITION 10 BrownBlue 14 BrownBlack 10